# General Operation Safety

- Due to entanglement risk, do not wear gloves.

- Use personal protective equipment. Always wear eye protection and foot protection. Protective equipment such as steel toe-capped shoes, safety glasses and hard hat will reduce personal injuries. Always wear personal safety equipment when performing the following actions:

  - Equipment cleaning

  - Maintenance or check ups

  - Eliminating blocking conditions

  - Adjustments

- The safety guards are included with the equipment and are intended to inhibit access to hazardous parts of the equipment when in operation. Any form of manipulation or modification is absolutely prohibited.

- In case of input pressure reduction, position the arm on the parking hook and turn off the device until the pressure has returned.

- Arm should be positioned on the parking hook at short-term interruptions.

- The payload must not change during operation.

- To stop the tool from functioning, turn the main switch of the tool control unit to the "OFF" position.

- At the end of the work day or prior to longer inactive periods of time, position the arm on the parking hook and close the air supply shut-off valve before shut down.