# Floor Properties

Torque Arms should be mounted to a surface with sufficient rigidity and support, to withstand torque reaction and total weight of Torque Arm assembly and tool.

Concrete slab thickness | 150 mm | 6 in | Minimum
Concrete compressive strength | C20/25 | 3000 lbf/in2 | Minimum
Aggregate size | 25 mm | 1 in | Maximum
Reinforcing quality | 500 Bst- Ductility standard (class A) bar ASTM A615 Grade 60 bar
Concrete slab area | 2.25 m2 | 3488 in2 |
Dimensions |
Width | 1500 mm | 59 in |
Length | 1500 mm | 59 in |
Concrete steel cross sectional area |
Area for X- and Y- direction | 188 mm2/m | 0.089 in2/ ft |

It is the responsibility of the end user to ensure that the floor conditions meet the indicated specifications. If a different fixing material (anchor) is chosen by the end user than what is specified, then it is their responsibility to ensure that the anchors are sufficient for the application. The appropriate installation instructions must be respected at all times.