# Arm Components Overview

Part | Description
--- | ---
A | Pillar
B | Adjustable Rotation Stop
C | Shoulder Joint
D | Boom Arm
E | Elbow Joint
F | Outer Parallel Arm
G | Inner Parallel Arm
H | Reaction Brake
I | Vertical Rod

## Arm Dimensions

After complete setup of the torque arm, a minimum 30 degree angle limitation is important to keep.

Part | Description | Length
--- | --- | ---
A | Vertical Travel - Pneumatic | 750 mm (29.5 in)
B | Working Radius - Pneumatic | 1460 mm (57.4 in)
C | Max Working Radius | 1557 mm (61.2 in)
D | Inside Working Radius | 151 mm (5.9 in)
E | Vertical Rod Mounting Height | 686 mm (27.0 in)