# Connecting to External PC using Windows Remote Desktop

1. Connect an Ethernet cable to the ILS Sensor's LAN 2 port.​ Connect the other end of the Ethernet cable to an external PC.​

2. Power on the ILS Sensor.

3. Open the Remote Desktop Connection app on the external PC.​

   - ​ Type in ivne-xxxxxxxx (where xxxxxxxx is the name of the ILS Sensor), and select Connect.

   - The sensor's name is the serial number and can be found on the product label.

4. Type in the password (isra) in the login window, and select Yes.

   The ILS Sensor and ILG Software run remotely on the external PC.

## Applies to:

8436 6771 00
8436 6771 01