# General Installation Safety

Sensor must be mounted to station overhead or floor post, but must not be effected by any station vibrations or tooling movements that may cause alignment change.

WARNING

Crushing Hazard

Use additional safety equipment to prevent the sensor from falling, causing property damage and/or bodily injury.

- Attach a safety wire with a safety hook to the safety eye on the sensor. Secure the safety wire to a rigid object.

## Applies to:

8436 6771 00
8436 6771 01