# Connecting to the Controller via the Factory Port

When the ILS Sensor is connected to the controller's factory ethernet port, the controller can not be connected to the customers Factory Network.

## Without Using Router or Ethernet Switch

1. Connect an Ethernet cable from the ILS Sensor's LAN 1 port to the factory Ethernet port of the controller.

2. Connect a second Ethernet cable from the ILS Sensor's LAN 2 port to an external PC.

3. Connect monitor, keyboard, mouse, and other accessories to the ILS Sensor's USB ports.

4. Check the IP settings of the controller.

5. Use the Remote Desktop Connection app to connect the external PC to the ILS Sensor. In the Remote Desktop Connection app, type in the name of the ILS Sensor:

   ivne-xxxxxxxx , where xxxxxxxx is the serial number of the ILS Sensor (printed on the label on the connector plate).

6. Go to Control Panel > Network and Internet > Ethernet > Change adapter options > LAN 1 properties > Internet Protocol Version 4 > Properties.

   Change the IP address for the ILS Sensor to the same IP-range as for the controller.

7. After finalizing the installation of ILG licenses the external PC can be disconnected from the workstation.

## Using Router or Ethernet Switch

1. Connect an Ethernet cable from the ILS Sensor's LAN 1 port to the router.

2. Connect a second Ethernet cable from the controller's factory Ethernet port to the router.

3. Connect the external PC to the router.

4. Connect monitor, keyboard, mouse, and other accessories to the ILS Sensor's USB ports.

5. Check the IP settings of the controller.

6. Open a web browser and type the IP address of the controller's Factory Ethernet port.

7. Use the Remote Desktop Connection app to connect the external PC to the ILS Sensor. In the Remote Desktop Connection app, type in the name of the ILS Sensor:

   ivne-xxxxxx , where xxxxxx is the serial number of the ILS Sensor (printed on the label at the connector plate).

8. Go to Control Panel > Network and Internet > Ethernet > Change adapter options > LAN 1 properties > Internet Protocol Version 4 > Properties.

   Change the IP address of the ILS Sensor to the same IP-range as of the controller.

9. After finalizing the installation of ILG licenses the external PC can be disconnected from the workstation.

## Applies to:

8436 6771 00
8436 6771 01