# Controller Connection Options

The ILS Sensor can be connected to the controller in the following ways:

- Via the controller's Factory Port. (Supported for Power Focus 6000, Power Focus 4000, and Power MACS controllers).

- Via the controller's COM Port. (Only supported for Power Focus 6000 controllers).

- Via the Factory Network. (Only supported for Power Focus 6000 controllers).

## Applies to:

8436 6771 00
8436 6771 01