# ILS Sensors

There are two types of receivers based on the type of application:

ILS Sensor Standard Workspace/ILS Sensor Wide Workspace

## ILS Sensor Standard

The standard ILS Sensor has a bolt accuracy of 10 mm and is used for standard applications.

## ILS Sensor Wide

The wide ILS Sensor has a bolt accuracy of 20 mm and is used for bigger area coverage.

## Structure of the Sensors

The ILS Sensor consists of two cameras, two infrared lighting units, and one computing unit.

Structure of the Sensor

## Applies to:

8436 6771 00
8436 6771 01