# Connector Plate Overview

Item | Description
--- | ---
LAN 1 | Ethernet connection for configurable IP address
LAN 2 | Ethernet connection for fixed IP address (default 169.251.1.1)
24V DC | Power inlet (135 W, 5.6 A)
SD card | The SD card is used for storing settings, and transferring configurations between different ILS Sensors.
HDMI | HDMI connections for displays
USB | USB connections for keyboard, mouse, scanners, and other accessories

## Status Light Indications

The status lights on the connector plate for the sensor provide the following information:

Symbol | Status Light Color | Description
--- | --- | ---
| Orange (blinking quickly) | Ethernet cable connected to LAN1 port and Ethernet connection established Sensor tracking-software running Communication works Data traffic
Green (continuous light) | Ethernet cable connected to LAN1 port and Ethernet connection established, but Sensor tracking-software not running
Red (blinking slowly) | Ethernet cable disconnected from LAN1 port and/or Ethernet connection could not be established
| Black (no light) | Sensor PC off Power failure of PC
Green (continuous light) | Sensor PC running, works normal
Green (blinking) | Sensor PC in standby
| Black (no light) | Sensor not powered (24 V DC not available) No power cable connected Power failure
Green (continuous light) | Power On (24 V DC available)

## Applies to:

8436 6771 00
8436 6771 01