# Installing the ILS Sensor

1. Before mounting the ILS Sensor, carefully consider the intended position. Keep in mind that the targets must always be visible to the cameras of the ILS Sensor.

2. Mount the ILS Sensor. Contact your local Atlas Copco representative for information on appropriate mounting brackets and installation instructions.

3. Connect the Ethernet cable to port LAN 1, or port LAN 2.

   Port LAN 1 is configurable, while port LAN 2 uses a fixed IP address (default is 169.251.1.1).

4. Connect additional equipment, such as keyboard, mouse, scanner, and accessories, to the USB ports.

5. Connect monitor(s) to the HDMI ports​.

6. Connect the 24V DC power supply cable to the ​24V DC port (135 W, 5.6 A).

7. To setup and configure the ILS Sensor, refer to ILG Software User Guide.

Relevant Information

- Cable Information
- Product Data

## Applies to:

8436 6771 00
8436 6771 01