# Specifying settings for SQS3 station

You must first navigate to Smart AMS Config.

SQS3 stations are not controlled by Smart AMS.

- Go to the Smart AMS Config address in your web browser by using the Open Smart AMS Config UI shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6395. Make sure to replace localhost with the actual IP address of the computer Smart AMS Config is running on.

- To switch to the Configuration section, click in the Navigation Panel on the left of the page. On mobile devices with a smaller screen, click your username in the upper right corner of the page, and then select Configuration.

- Click the icon of the SQS3 station.

Inactive toggle switch: If this toggle switch is turned on, the station is inactive. The icons of inactive stations appear dimmed. Inactive stations are unavailable for Smart AMS; they are ignored. If turned off, the station is activated.

Station name field: Specify the name of the station.

Station number field: Specify the ordinal position of the station in the assembly line. Examples: 1, 2, 3.

Description (English) field: Provide a description for the station in English.

Description (local) field: Provide a description for the station in your local language.

SQS Station IP field: Specify the IP address for connection.

Is Rework Station toggle switch: If turned on, the station is considered as an SQS3 rework station. Otherwise, the station is considered as a regular SQS3 station.

Use line PLC sign-in toggle switch: If the product is to be signed in by the line PLC, turn this toggle switch on. If no line PLC is used, turn it off.

Rework Station list: Select the station dedicated for product rework. It can be an SQS3 Rework Station. Otherwise, select Not set.