# Adding a recipe

You must first navigate to Smart AMS Config.

- Go to the Smart AMS Config address in your web browser by using the Open Smart AMS Config UI shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6395. Make sure to replace localhost with the actual IP address of the computer Smart AMS Config is running on.

- To switch to the Configuration section, click in the Navigation Panel on the left of the page. On mobile devices with a smaller screen, click your username in the upper right corner of the page, and then select Configuration.

- Click the icon of the Smart AMS station for which you want to add the recipe, and then click Recipes.

- Click Add recipe. To add another recipe, click Add recipe again.

Bolt Case name field: Type the bolt case name—the text string which is a unique identifier of the bolt case within all stations and recipes. This is part of outward information for bolts.

Bolt Case description field: Enter a description for the bolt case.

PR Combination field: Restrict the recipe to a specific combination of PR Codes. To accept all workpieces, leave this field blank.

Controller list: Select the controller to be used.

Program number field: Specify the tightening program number.

Tightening count field: Specify the number of bolts that you want tightened using the specified tightening program.

Spindle count field: Specify the number of spindles used with the tool. A wrong number will affect the output data for bolts, because bolt case names will not be correctly mapped to the results. For example, if Tightening count is set to 3, and Spindle count is set to 2, this means there are 6 bolts in the configuration.

MNO count field: Specify the maximum amount of consecutive NOK retries. The counter is reset to 0 when an OK tightening is performed. It starts counting when a tightening attempt is NOK. For unrestricted number of retries, leave the field empty.

Area ID field: Specify the identification of the ILT area pertaining to the station. The ILT-driven tools at the station will only be enabled when inside the area. If this field is left blank, the tool specified in the recipe will be enabled regardless of its position.