# Mapping features

After your purchase, you can map the available features to Error Proofing License Manager.

Ensure that you have Internet connectivity from the computer running Error Proofing License Manager.

- Log on to https://atlascopco.flexnetoperations.com/control/atco/login

- Click the Search License Manager or USB Device link, and then find your record by entering the ID, device name, or site name.

  You will see a list of entries.

- Click the corresponding ID in the list. You will be switched to the View License Manager or USB Device page.

- On the View License Manager or USB Device page, click the Map Features link.

  You will see a list of features. You can filter the list by using the available criteria and clicking the Search button.

- In the Qty to Add column, specify the number of feature instances you want to add to your Error Proofing License Manager, and then click Map Features.

After some time, the features will appear in your Error Proofing License Manager. The refresh interval is configured on the Properties page in Error Proofing License Manager.

Parameters that affect mapping

Server host ID: Select the MAC address that you used when registering Error Proofing License Manager.

Synchronization to Backoffice Interval: The amount of time between synchronization sessions with the back office. Example: 10m (for ten minutes). A low amount can place a load on the server.

Capability Polling Interval: The amount of time between capability-request polls. Example: 10m (for ten minutes). A low amount can place a load on the server.