# Specifying settings for Smart AMS station

You must first navigate to Smart AMS Config.

- Go to the Smart AMS Config address in your web browser by using the Open Smart AMS Config UI shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6395. Make sure to replace localhost with the actual IP address of the computer Smart AMS Config is running on.

- To switch to the Configuration section, click in the Navigation Panel on the left of the page. On mobile devices with a smaller screen, click your username in the upper right corner of the page, and then select Configuration.

- Click the icon of the Smart AMS station you want to configure, and then click General.

Inactive toggle switch: If this toggle switch is turned on, the station is inactive. The icons of inactive stations appear dimmed. Inactive stations are unavailable for execution of work; Smart AMS ignores them. If turned off, the station is activated.

Station name field: Specify the name of the station.

Station number field: Specify the ordinal position of the station in the assembly line. Examples: 1, 2, 3.

Description (English) field: Provide a description for the station in English.

Description (local) field: Provide a description for the station in your local language.

Product sign-in list: Specify how to sign in products at the station.
PLC: Products can only be signed in by PLC.
Barcode: Products can only be signed in by barcode scanner.
PLC & barcode: Products can only be signed in by either PLC or barcode scanner.
MES: Products can only be signed in by MES.
MES & barcode: Products can only be signed in by either MES or barcode scanner.

Execution mode list: In case of multiple tools, it determines the sequence in which the tools operate: parallel or sequential.
In parallel execution mode, if there are multiple tools at the station, the operator or operators may use the tools simultaneously—all tools specified in all recipes for the station will be active simultaneously. For this, select Parallel.
In sequential execution mode, tools can only be used in the order in which the recipes are listed. For this, select Sequential.

Rework Station list: Select the station dedicated for product rework. It can be an SQS3 Rework Station. Otherwise, select Not set.

LAN Scanner

Enabled toggle switch: If turned on, LAN scanner is used. Otherwise, no LAN scanner is used.

IP field: Specify the IP address for connection. Use this setting if you have a LAN scanner connected to the Smart AMS Server. Otherwise leave this field blank.

Port field: Specify the port for connection. Use this setting if you have a LAN scanner connected to the Smart AMS Server. Otherwise leave this field blank.

Product idle timeout

Override global setting toggle switch: If you want to override the global setting for product idle timeout at the station, turn it on. Otherwise, turn it off.

Product idle timeout field: Specifies the time period, in seconds, to wait until the product is signed out due to inactivity. After the idle timeout is reached, the product will be signed out in the NOK state. To deactivate this function, leave the field blank.