# Removal of Jammed Screws

Follow the below troubleshooting steps to remove the Jammed Screws:

- Never use excessive force for removing the jammed screws.

- By opening the Alignment Jaws or lifting the Swivel Arm up, the jammed screws comes out easily from the feeding head.

- In case of timing issues, the screws get struck between the Bit and the down holder. Adjust the timing in the software of the Feeder. Find more information in the Screw Feeding Unit Manual.

- To dislodge the jammed screws, the air supply should be turned OFF and the Feeding Head should be removed from the tightening module. This procedure eliminates force to the tool parts and the screws get easily removed.

- Find more information in the chapter on Removing and Replacing the Feeding Head.

## Applies to: