# Removing the Bit and Bit Adaptor

## Removing the Bit from the Threaded Sleeve

1. There are two ways of removing the Bit from the Threaded Sleeve.

   - Hold the Threaded Sleeve with the Hook Wrench, and use pliers to unscrew the Bit from the Threaded Sleeve.

   - Another method is to clamp the Bit and unscrew the Threaded Sleeve with the Hook Wrench.

2. Perform step 1 in the reversed order to attach the new Bit to the Threaded Sleeve. Make sure that the Bit is not damaged during this procedure.

3. Make sure that the Bit, Threaded Sleeve, and new Bit Adaptor are correctly mounted together.

4. Insert the Bit Assembly into the Screw Feeding Front Part using the Bit Quick-change Coupling.

Positions | Components
1 | Hook Wrench
2 | Threaded Sleeve
3 | Mounting Tool
4 | Bit Adaptor
5 | Bit

## Removing the Bit Adaptor

1. Hold the Threaded Sleeve with the Hook Wrench and make sure the hooks are into the holes.

2. Use the Mounting Tool to grip the Bit Adaptor and release it from the Threaded Sleeve.

## Tightening Torque Specifications

Dimension | Tightening Torque (Nm)
M4 | 3
M5 | 6
M6 | 10
M8 | 25

## Applies to: