# Maintaining the Driving Tool

Follow the below steps to maintain the Driving Tool:

- For maintaining the tool, it has to be disassembled from the stroke unit.

- Remove the screws on the adapter plate and pull the driving tool out.

- The Driving Tool can now be maintained as described in the Tool´s product manual.

- After maintaining the tool lubricate the drive shaft and assemble the driving tool to the stroke unit. For Lubrication of the drive shaft (1) use Klüber Paste 46MR401.

No. | Component | Function
1 | Drive Shaft | Geared shaft of the rotary drive

## Applies to: