# Cleaning and Lubrication of the Stroke Rail Carriers

Follow the below instructions to clean and lubricate the stroke rail carriers:

- Clean the stroke rails using a wipe and industry cleaner and remove all impurities.

- Lubricate the rail carriers by using a grease gun filled with Klüber Isoflex NBU 15.

- By moving the carrier, the lubricate nipples will become reachable for the grease gun.

- Inject 3-5 strokes of the grease in all lubricant nipples and remove any leaked grease.

## Applies to: