# General Installation Safety

- Always make sure that the drive unit/controller is switched off before connecting/disconnecting the tool cable.

- Always disconnect the tool from the drive unit/controller before making any adjustments on or inside the tool.

- The tool with its drive/controller box is designed to operate at any setting within its torque range at a primary voltage of nominal 230V/ 50Hz alternatively 115V/ 60Hz, single phase. Refer to the manual for the drive unit or controller.

- Make sure that the tool is in good working order and that the controller is correctly programmed before use to avoid unexpected behavior from the tool which may result in operator injury.

## Applies to: