# Operation

In this chapter, the operational safety instructions, general instructions for the operator, and the workflow of the module are described.

Please read the below safety instructions before Operation.

WARNING

Moving parts Hazard – Feeding Tubes

Unexpected pneumatic movements of the feeding tubes cause outflows of screws at high speed. This may lead to severe injuries especially to the eyes.

- Always verify that all connections between the Feeding Tube and the Swivel Arm are securely fastened before pressurizing the tool.

  The pneumatic power supply must be switched off and vented during all work on the Screw Feeding Tightening Module.

  Always make sure that there are no damages or loose feeding tubes or fittings.

  Always shut off the air supply, drain hose of air pressure, and disconnect tool from air supply when not in use, before changing accessories or when making repairs.

  Never direct air at yourself or anyone else.

  Whenever universal twist couplings are used, lock pins must be installed.

WARNING

Occupational Entanglement Hazard

Choking, scalping or other severe bodily injuries can occur if loose clothing, jewellery, neck ware, and hair is not kept away from tool or accessories.

- Never operate the tool wearing loose objects.

- Never wear gloves when operating the tool.

- Keep loose clothing, jewellery, neck ware, and hair away from rotating drive or accessories.

WARNING

High Pressure Hazard

Due to damaged or inadequately inserted compressed air hoses into the couplings, air can escape under high pressure and may cause injury to the eyes.

- Regularly check the feeding tubes for damage.

- In the case of damage to the pneumatic components, the system must be switched off immediately, de-aerated and secured against being switched on again. And, proceed to repair.

## General Instructions for the Operator

- Make sure you are familiar with the operator’s instructions before you use this tool.

- The tool together with any attachments or accessories, must never be used for anything other than the designed purpose.

- All locally legislated safety rules regarding installation, operation, and maintenance shall be respected at all times.

- This product is only intended for industrial use and shall only be operated indoor in dry rooms. This product must not be used in explosive atmospheres.

- Keep hands, long hair, and other objects away from the rotating socket.

- Make sure that the tool is in good working order and that the controller is correctly programmed before use to avoid unexpected behaviour from the tool which may result in operator injury.

Do not use force when handling the Screw Feeding Tightening Module.

Use only accessories recommended by the manufacturer. The connection of unsuitable accessories is a potential source of danger.

Check the Screw Feeding Tightening Module for any incorrect adjustments, jammed moving parts, damage, and other faults that could affect the operation of the device.

## Applies to: