# Maintaining the Feeding Head

## Removing and Replacing the Feeding Head

The Feeding Head needs to be repaired in case of damage. An inadequately maintained Feeding Head is a source of danger.

Follow the below steps to remove and replace the Feeding Head:

- Push the Swivel Arm aside and pull the sleeve of the Quick-change Coupling backwards, and then pull off the Feeding Head (in blue color).

- Attach the clean or the new Feeding Head and then release the sleeve of the Quick-change Coupling.

- Make sure that the Feeding Head is correctly attached by turning and pulling it gently. The Feeding Head should remain attached to the tightening module.

## Cleaning and Checking the Feeding Head

- Clear the dirts of the Feeding Head using an industrial cleaner and a cloth.

- Inspect the Feeding Head visually and check for damage. If damaged, the Feeding Head or the damaged components must be replaced.

## Applies to: