# Packaging and Storage

## Packaging

The packaging is intended to protect the individual components from transport damage, corrosion, and other damage during transport until assembly. The packaging must not be damaged under any circumstances and should only be removed immediately before assembly.

## Storage

The devices and, if necessary, spare parts should be stored in a packaged condition, which provides further protection against environmental influences. The following conditions for storage must be observed.

- Never store outdoors - not even for a short time.

- The components should be stored in a dry place, and should be protected from dust and aggressive media.

- Protect from sunlight.

- Avoid mechanical vibration.

- Storage temperature: + 10 ° C to + 55 ° C. High variations of temperature should be avoided.

- Relative humidity: 5% to 95% (not condensing).

- If the device is stored for longer than a month, the condition of all parts and the packaging should be checked regularly, if necessary, refresh/renew the preservation.

## Applies to: