# Replacing the Alignment Jaws

Follow the below steps to replace the Alignment Jaws.

- The Alignment Jaws must be replaced in case of wear or damage.

- Disassemble the Feeding Head by releasing the clamps and removing the stud.

- Replace the Alignment Jaws and assemble the Feeding Head.

- Using the alignment jaw device and the pin punch to drive the pins out.

- Replace the front part of the alignment jaws and use the alignment jaw device to hold the parts together when driving the pins back in.

## Applies to: