# Tools and Mounting Devices

## Required Standard Tools and Specifications

No. | Tools | Specifications
1 | Allen key | 1,5; 2, 2,5; 3; 4; 5; 6; 7; 8; 9; 10 (mm)
2 | Wrench | 5; 7; 8; 10; 13; 14; 17; 19; 22; 24; 26 (mm)
3 | Screw Driver | Set of Screw Drivers
4 | Diagonal Cutter |
5 | Torque Wrench | Up to 50 Nm
6 | Grease Gun | For guide block greasing
7 | Hot Air Gun | T=130°C
8 | Tube cutting tool | 4 to 35 mm

## Required Mounting Devices and Description

Mounting Devices | Description
Adjustable Hook Wrench | Tool for changing the Bit adaptor, Bit, and union nut of the stroke module.
Alignment Jaw Fixture | Device for fixing the tension pins with which fasten the alignment jaws to the holder. There are 2 holders and 2 mounting sides for the alignment jaws with different sizes: Left side: 7.0-9.0 mm Right side: 10.0-12.0 mm Left side: 13 mm Right side: 16 mm
Pin Punch | Tool for dismounting the tension pins which hold the alignment jaws in the holders.
Holder with the spline | Holder with the spline is used to change the Bit. During Bit-change, the adaptor should be clamped securely.

## Applies to: