# Intended use of the Fixtured Tightening Module

This product is designed to feed and hold the screws in position and apply the specified Torque to the joint in an automated process. The tightening process is controlled by the Power Focus 6000. No other use is permitted.

The partly completed machine is a fixtured screw feeding system intended for producing screw connections. The screw feeding is proceeded automatically by a Screw Feeding Unit. The Fixtured Screw Feeding Tightening Module and the Screw Feeding Unit are powered and controlled by the Power Focus 6000 and customer PLC (Programmable Logic Controller).

- The tightening module should be used only indoors.

- The tightening module should be put into operation only with the system components described here.

## Permitted use of the Fixtured Tightening Module components

- Fixtured Tightening Module and Driving Tool - Requires a defined torque or a defined angle of rotation.

- Cables (electrical) - Provides electrical supply and controls the screw fastening system.

- Hoses (pneumatic) - Supplies the Fixtured Tightening Module with pneumatic energy from the Screw Feeding Unit.

- Feeding Tube - Transports fasteners from the Screw Feeding Unit to the feeding head.

- Power Focus 6000 - Controls and monitors the screw fastening process.

- Screw Feeding Unit - Feeds the Fixtured Tightening Module with screws.

## Applies to: