# Installing the ILS Target

1. Remove the T10 screw and the cap.

2. Remove the cover tags.

3. Remove the four T8 screws so that the two holders underneath become loose.

4. Fasten the two holders onto the tool.

5. Mount the ILS Target onto the holders.

6. Tighten the four T8 screws.

7. Insert the ILS Matrix cards.

   Make sure to insert the side with the clipped corners first.

   Be careful not to scratch the surface of the ILS Matrix. It can affect the performance of the positioning.

8. Put the cap back and tighten the T10 screw.

9. Only applicable to TBP tools: Put on the rubber cover.

## Applies to: