# Specifying settings for SQS3 station

You must first navigate to Smart AMS Config.

SQS3 stations are not controlled by Smart AMS.

- Go to the Smart AMS Config address in your web browser by using the Open Smart AMS Config UI shortcut on the Desktop or on the Windows Start menu.
  Sample address: http://localhost:6395. Make sure to replace localhost with the actual IP address of the computer Smart AMS Config is running on.

- To switch to the Configuration section, click in the Navigation Panel on the left of the page. On mobile devices with a smaller screen, click your username in the upper right corner of the page, and then select Configuration.

- Click the icon of the SQS3 station.

Inactive toggle switch: If this toggle switch is turned on, the station is inactive. The icons of inactive stations appear hatched. Inactive stations are ignored. If turned off, the station is activated.

Station name field: Specify the name of the station.

Station number field: Specify the ordinal position of the station in the assembly line. Examples: 1, 2, 3.

Description (English) field: Provide a description for the station in English.

Description (local) field: Provide a description for the station in your local language.

SQS Station IP field: Specify the IP address for connection.

Is Rework Station toggle switch: If turned on, the station is considered as an SQS3 rework station. Otherwise, the station is considered as a regular SQS3 station.

Use line PLC sign-in toggle switch: If the product is to be signed in by the line PLC, turn this toggle switch on. If no line PLC is used, turn it off.

Rework Station list: Select the station dedicated for product rework. It can be an SQS3 Rework Station. Otherwise, select Not set.

## Applies to: