# Maintenance Intervals

Under normal operating conditions, with an 80% load and maximum motor temperature of 80 °C, service the tool at the following intervals:

Tool Type | Maintenance Interval
--- | ---
Angle | Every 250,000 cycles.
Straight | Every 1 million cycles or once a year, whichever comes first.
Offset | Every 1 million cycles or once a year, whichever comes first.

If the tool is operating in tougher conditions than those above, please contact the local Atlas Copco Service Center for specific maintenance interval information.