# Installation Overview

This tool can be installed by using the front screw holes. See the dimensional drawings on ServAid for installation dimensions.

Torque table
Screw | Torque [Nm] | Torque [ft·lb]
--- | --- | ---
M3 | 1.7 | 1.25
M4 | 4.0 | 2.95
M5 | 7.5 | 5.53
M6 | 13 | 9.59
M8 | 30 | 22.13
M10 | 60 | 44.25
M12 | 110 | 81.13
M14 | 180 | 133
M16 | 280 | 206.52

Oil the threaded parts of the screw before tightening.

Only use screws with strength class 12.9 (DIN 912).