# Installing the Motor Cable

WARNING

Electrical hazard

Turn off mains power supply before adjusting or servicing.

1. Align the motor cable with the pins on the tool contact.

2. Push the motor cable gently towards the beginning of the threads.

3. Turn the handle (A) clockwise to install and lock the motor cable.

NOTICE

Tool Damage

The contact pins will be damaged if they are not aligned.

- Do not use excessive force to insert the tool motor cable.