# Main components and functions

This product, its attachments and accessories are intended to be used for drilling, reaming, and countersinking.

Pos | Component | Function
--- | --- | ---
1 | Chuck guard | Secures the precision while maintaining a comfortable grip.
2 | Chuck | Inserts and keeps the drill bit (cutter) in position.
3 | Spacer ring | Used for dismantling the chuck.
4 | Gear unit | Gears up the torque from the air motor.
5 | Trigger | Starts the drill with slow start function.
6 | Lubrication free air motor | Gives a cleaner working environment.
7 | Handle | Gives a comfortable rubber grip.
8 | Inlet adapter | Connects the drill to the air preparation unit (pressurized air).
9 | Adjustable air exhaust | Guides the cool air away from the operator.