# Export Configuration

The export function is used to export tightening results accessible in the Reports menu for analysis in external programs.

The export function is used to:

- Export tightening results and events for further processing from the cable tool.

- Export log files for debug assistance from an Atlas Copco service engineer.

- Export controller configuration that can be used to copy settings to another controller.

In this Section

- Exporting Data from the Mobile GUI
- Exported Files
- Exported .csv File Format