# TC - Torque Calibration

Tools
QST

This step is only supported for dual transducer tools.

The Torque Calibration step runs the tool with the specified speed in the forward direction until the torque target is reached.

Parameter | Description
--- | ---
Target torque | Must be > 0.
Speed | Must be > 0. Default: 60 rpm.
Transducer | Main or Secondary. Default: Main. Set to Secondary in order to calibrate the front transducer.
Adaptive brake (Valid only for Power Focus 6000 StepSync, Power Focus 8 StepSync, and Flex). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.