# Configuration of the Network

The Power Focus XCPower Focus XC can be set up for access from the Atlas Copco software ToolsTalk or from a web browser on a Local Area Network (LAN). It can also be accessed directly from a connected PC. It uses the IPv4 protocol.

To access and alter the Ethernet settings, select Edit.

Only the Factory Ethernet port can be configured. The Service Ethernet port has a designated IP address, 169.254.1.1, that must not be connected to the local network.

In this Section

- Accessing the Controller On Lan
- Accessing the Controller Through a Web GUI
- Accessing the Controller Through a Mobile GUI