# Exporting "All Controller Information"

It is possible to export controller configuration, settings, results, and events for further processing. Part of the export is done both from the cable tool, as well as connected wireless tools.

All data included in the export is stored in a file "PFExport_<IAM name>_<datetime (lowest value displayed for time is seconds)>.tar.gz", which includes the following files and directories:

- "PFExport_<datetime>_Results.csv" – All available results

  The results are exported in a CSV formatted text file. The latest performed result is the first in the CSV file.

  It is possible to export the following result information for tightenings and loosenings:

Result Information | Power Focus XC - Tightening Programs | Power Focus XC - Multistep Programs
--- | --- | ---
Identity number | - | -
Type of tightening | X | X
Virtual Station name | X | X
VIN (Identifier String) | X | X
Date and Time | X | X
Unique tool identifier | X | X
Batch Sequence Name | X | X
Batch Sequence Counter | X | X
Batch Count | X | X
Bolt name | - | -
Total status | - | -
Total status info | - | -
Status | X | X
Status info | X | X
Mode Name | - | -
Tightening program/Multistep Name | X | X
Stopping error | - | X
Errors | - | X
Failing Step | - | X
Channel | - | -
Target Torque (Nm) | X | X
Final Torque (Nm) | X | X
Target Angle (deg) | X | X
Start Final Angle (Nm) | X | X
Final Angle (deg) | X | X
Rundown Angle (deg) | X | -
Residual torque correlation factor | X | X
Elapsed time (s) | - | X
Angle low limit (deg) | X | X
Angle high limit (deg) | X | X
Torque low limit (Nm) | X | X
Torque high limit (Nm) | X | X
Number of pulses | X | -
Current at shutoff (A) | X | X
TrueAngle compensation (deg) | X | X
Time to rundown complete (ms) | X | -
Time to final torque (ms) | X | -
Target Text | X | X
Step Data | - | X
Selftap Torque | X | X
Prevailing Torque | X | X
Rundown Angle Trigger | X | X

The field delimiter and number format depends on the language settings:

Language | Date/time | Field delimiter | Number format
--- | --- | --- | ---
English (en_US) | MM/dd/yyyy hh:mm:ss | , | 123.456
Czech (cs) | dd.MM.yyyy hh:mm:ss | ; | 123,456
German (de_DE) | dd.MM.yyyy hh:mm:ss | ; | 123,456
Spanish (es_ES) | dd/MM/yyyy hh:mm:ss | ; | 123,456
French (fr_FR) | dd/MM/yyyy hh:mm:ss | ; | 123,456
Korean (ko_KR) | yyyy-MM-dd hh:mm:ss | , | 123.456
Italian (it_IT) | dd/MM/yyyy hh:mm:ss | ; | 123,456
Japanese (ja_JP) | yyyy/MM/dd hh:mm:ss | , | 123.456
Portugese (pt_BR) | Dd/MM/yyyy hh:mm:ss | ; | 123,456
Russian (ru_RU) | dd.MM.yyyy hh:mm:ss | ; | 123,456
Swedish (sv_SE) | yyyy-MM-dd hh:mm:ss | ; | 123,456
Chinese (zh_CN) | yyyy/MM/dd hh:mm:ss | , | 123.456

- "PFExport_<datetime>_Events.csv" - All available events

  The following event information are exported in a CSV formatted text file:

  - Severity

  - Date

  - Time

  - Code

  - Description

  - Virtual Station that triggered the event (only exported for PFXC-Handheld)

- "/settings" - Settings and configurations (used by Import)

- "jsonConfigurations.zip" - Multistep Tightening and Loosening programs are exported as .json files (to be used with MID2500)

- "atlas_sys_d.zip" - Logfiles from Drive application

- "atlas_sys_i.zip" - Logfiles from IT application

- "atlas_protocol_log.zip" – Logfiles from external protocol adapters

- “ExportInfo.txt” - Text document containing information about the IAM and Controller

- "atlas_plc.zip" - PLC configuration

- “licenseInformation.zip” – License Information and System Capabilities

## How to Export "All Controller Information"

1. On the Home view, select the Controller Tab. Then, on the left side, select the Export/Import Tab .

2. In the Export window, open the drop-down menu and select All controller information.

3. In the Export window, select Export.
   At the end of the exporting process, an exporting pop-up window confirms that the export is done.
   A PF/IXBExport_<IAM name>_<datetime>.tar.gz file is automatically downloaded.