# TC - Torque Calibration

Tools
QST

This step monitor is only available for tools equipped with dual transducers.

The Torque Calibration monitor checks if the maximum torque reached is within the torque limits.

Parameter | Description
--- | ---
Transducer type | Main or Secondary Set to Secondary for the front transducer of the tool.
Low limit | Must be >= 0
High limit | Must be > 0 Must be > Low limit