# Quick Start Guide

To provide a better overview of the system, the following instruction touches upon the steps that are required to start using the system.

The instruction does not cover all system features, but focuses on the most basic.

## Web GUI

1. Select the type of tool to use. The tightening strategies available, depend on the type of tool you select.

2. Set a Tightening program that contains all relevant parameters, for example target angle and target torque. The main purpose of the tool is to perform a tightening.

3. Create a Virtual station and assign a tool to it. The virtual station acts as an interface between the controller and the tool, so several tools can be connected to a single physical controller. A virtual station is always required, even if only one tool is connected to the controller.

4. Assign a task to the Virtual station. The task can be either a tightening program, or a specified digital input (from for example a barcode scanner). The tool assigned to the station will now be able to perform the task.

## Mobile GUI

1. Select the type of tool to use.

2. Create a tightening Task and set the relevant parameters, for example target torque and target angle. The main purpose of the tool is to perform a tightening.

3. The created task will be assigned to a virtual station. The tool assigned to the station will now be able to perform the task.