# T|A – Tighten to Torque or Angle

Tools
ES STR SL ST SR QST STB IXB

This step runs the tool with the speed n in the forward direction until the first of either torque target or angle target is reached. The torque and angle measurements start at the beginning of the step.

Parameter | Description
--- | ---
Target torque | Must be > 0.
Target angle | Must be > 0.
Speed | Default: 60 rpm. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Brake (Valid only for Power Focus 6000 StepSync, Power Focus 8 StepSync, and Flex). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

Point and click on image to see more information:

A | Target Torque
B | Target Angle