# PTCA - Post Thread Cut Angle

Tools
ES STR SL ST SR QST STB IXB

Measures the angle achieved during the monitoring and checks that it is between the specified angle limits. The Trigger Torque level is ignored until the end of the Thread cut angle window is reached. After that, the angle measuring starts as soon as the measured torque is above Trigger Torque. The parameter Stop Condition specifies where the angle measurement should end.

Parameter | Description
--- | ---
Trigger torque | Must be >= 0
Thread cutting angle window | Must be > 0
Angle measurement type | Peak angle Angle at peak torque Shut off angle Angle at end
Thread cut trigger torque | Must be >= 0
Low Limit | Must be >= 0
High Limit | Must be > 0 Must be > Low limit