# Export/Import

The Export/Import Tab supports the user to make one of the following operations: Export, Import, and Automated backup.

The Export window supports the user to export controller configurations, settings, results, and events. In addition, it is possible to export tool logs, which can be shared with Atlas Copco Service personnel to troubleshoot problems with the tool(s).

The Import window supports the user to import controller configurations and settings.

It is only possible to have one active Export or Import at the time. Any attempt to start a new Export/Import while there is an ongoing Export/Import is rejected.

The Automated backup window supports the user to generate automatically a backup file.

It is possible to export data by using:

- Web GUI

- ToolsTalk 2

- Mobile GUI (export to device)

- USB flash drive, in Mobile GUI

The USB flash drive needs to be formatted and with a partition to work for Linux: possible formats are, for example, FAT or NTFS.

It is possible to import data by using:

- Web GUI

- ToolsTalk 2

During the Export/Import process a progress bar informs the user that an export/import is ongoing. The time to perform an export/import is depending on the numbers of results, events, and log files.

## Export/Import Between Controllers

Controllers may have different IAM types that could have different capabilities.
A controller can export all the configurations that are applicable for the current type of IAM module.

A controller cannot import a file exported from a different type of IAM module. This is applicable also when using ToolsTalk 2.

In this Section

- Exporting "All Controller Information"
- Exporting "Settings and Configurations"
- Exporting "Logs from Connected Tools"
- Exporting "Results"
- Exporting "System Logs and Information"
- Importing Controller Configurations and Settings