# Tool Disabled - 158

Tool Disabled is an output signal which is activated when the tool is externally disabled by any of the following signals:

- 20002 - Lock Tightening

- 20003 - Lock Loosening

- 20004 - Lock Tool Active High

- 20033 - Line Control Lock

- 20018 - Open Protocol Lock

- 20020 - Fieldbus Lock Tightening

- 20021 - Fieldbus Lock Loosening

- 20040 - Soft PLC Lock Tightening

- 20041 - Soft PLC Lock Loosening

- 20061 - Lock Tool Active Low

Name in SoftPLC: TOOL_DISABLED

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE