# Accessing the Controller On Lan

Select the Network menu and on the Factory Ethernet Port window, click Edit. Then, set Enabled to On to alter the Ethernet settings.

Connect the network cable to the Factory Ethernet port and then either manually specify the required information or, if available, use the information provided by the DHCP server. Required information is:

- IP address

- Subnet mask

- Gateway

This information is provided by the local system administrator.

When using the manual option there are optional settings available for the use of DNS servers.