# A - Angle

Tools
ES STR SL ST SR QST STB IXB MWR-TA

This step monitor measures the maximum angle reached during the monitor and checks that it is between High limit and Low limit. The angle measurement starts at the start of the monitor or, if specified, at the point where the torque passes Trigger torque for the first time during the monitor.

Parameter | Description
--- | ---
Type | Four angle types are available: Peak angle (default), Angle at peak torque, Shut off angle, and Angle at end.
Trigger torque | The angle measurement starts at this trigger.
Low Limit | Lowest acceptable angle.
High Limit | Highest acceptable angle.