# External Result

External result is a strategy used when an OK tightening is indicated by an external digital signal (and not by torque or angle values measured during tightening).

When the signal is sent, the Result view will show the value of the Target parameter provided in the tightening program (specified torque value, angle value, or text string). These (torque and angle) values do not represent actual measured values, but only inserted text.

Parameter | Description | Default value
--- | --- | ---
Torque <Target torque> | Numerical value for desired displayed target torque value | 0.00
Angle <Target angle> | Numerical value for desired displayed target angle value | 360°
Text | Alphanumerical string for desired displayed text. |

In this Section

- Running the External Result Tightening Strategy with a Tool Connected