# Set up for M12 cable

The M12 cable is connected to two different connectors on the PF6 Flex system according to the table:

Connection from M12 cable(black) to Atlas special connector :
8-pin M12 A-coded male | Pin Num | 4-pol 240mm Black (PUR) | Pin Num
E - stop 1 | 1 | Brown | 6
E - stop 1 | 2 | White | 5
E - stop 2 | 3 | Blue | 4
E - stop 2 | 4 | Black | 3

Connection from M12 cable(Grey) to PCB connector.Manufacturing Article num: 1916371.

8-pin M12 A-coded male | Pin No | 4-pol 320mm Grey (PVC) | Pin num
Common | 5 | Brown | 1
Direction | 6 | White | 7
Start | 7 | Blue | 8
- | Not connected | Black | -