# Safe Storage

When the work is finished, make sure the following is done:

- The pressure is completely released from the tensioner which means it shows zero pressure on the hand controller and also on the analogue gauge of the pump.

- Take a backup of all reports before leaving site.

- The bar codes of the flange or other identifiers were scanned or noted related to the tightening results.

- In case of no bar code is available, the manual bar code can be entered.

- Mark the last completed bolt in case of a short break.

- Disconnect the pump from the main supply during overnight.

- Use the black cap on the pump inlet during transportation. It prevents oil from spilling during transit up and down the tower.

- Always use the certified lifting point on the frame marked at the back of the tensioner.

  Point and click on image to see more information:

  1 | Certified lifting point

- Cover the electronic connectors on the tensioner and the pump with dust caps.

  Point and click on image to see more information:

  1 | Electronic connectors covered with dust caps

  Point and click on image to see more information:

  1 | Electronic connector covered with dust cap

- Change the pump oil if the ambient temperature changes or if the pump is left unused for more than 90 days.

- Put all articles back in the respective boxes in the allocated positions.

## Applies to: