# SP2000 Hydraulic Power Pack

Point and click on image to see more information:

1 | Hydraulic coupling
2 | Oil filing neck (red cap)
3 | Certified lifting point

Locking ring on hydraulic coupling
Point and click on image to see more information:

1 | Phase rotation slot

Important:

- Check the oil level since it can drop at first start which will cause the system to stop if it is too low. Top up with the same grade of oil.

- Use the correct cap, black or red accordingly. The black cap for transportation, the red cap when the pump is in use.

- Power supply is 400V, 50/60 HZ, 3 phase. If no pressure builds up the first time, change phase by rotating the pins inside the socket.

- Make sure to lock the coupler after engagement.

- The system cables can be connected from any of two ends. To lock the system cable to the connector, push until it clicks. To remove the cable, twist and pull.

## Applies to: