# BCV - Clutch Type Battery Nutrunner

The clutch type battery nutrunner, model BCV BL-30-10 has range 10-30 Nm.

Point and click on image to see more information:

1 | Bright LED Illuminates the application in the dark
2 | LEDs For visual feedback
3 | Buzzer For additional feedback
4 | Trigger
5 | Battery The position is flexible, it can be reversed
6 | Ergonomic handgrip Reduces user's fatigue
7 | Direction switch Single press

Important:

- Check battery status by removing the battery and pressing the button inside.

- To change direction, press the direction switch button shortly and release, do not hold it for long. Holding the direction switch button for longer than 3 seconds can change its function.

- To remove the nutrunner from the tensioner, use the disengage key.

For more information about BCV, please visit https://servaid.atlascopco.com/AssertWeb/en-US/AtlasCopco/Catalogue/2247

## Applies to: