# STT - Smart Tentec Tensioner

Point and click on image to see more information:

1 | Lifting point
2 | Engagement for the battery nutruner
3 | Engagement point for the click wrench
4 | Hydraulic connection
5 | Pressure sensor Torque transducer Angle sensor
6 | Status indicators

Important:

- The eye bolt on the frame is a secure lifting point.

- Overshooting the click wrench can damage sensors.

- Avoid pressurised hose movements.

- Before transportation, remove the nutrunner and the click wrench.

- Stop the operation immediately in the event of oil leakage.

- Do not use any other tools as a replacement for nutrunner and click wrench.

## Applies to: