# Batch Assembly Mode - Program 2

Program 2 is optional and specific for particular applications.

1. On the Tasks tab on the hand controller, select Batch assembly, then select Program 2.

2. Scan the bar codes and accept it by pressing the forward button. There is an option for adding the bar codes manually by pressing the center button and selecting the manual input.

3. Enter batch count, then select the bolt position number on Position tool on bolt.

4. Start the program and follow the instructions at the bottom of the screen.

5. Follow the same procedure as for Batch assembly mode - First pass: Installation phase, Pressurization phase with nut rotation, and Pressure release.

6. When program 2 is completed on all bolts, batch will end and the main screen will appear. At this stage a report from the system can be generated.

## Applies to: